Selective Mirror (Selective data protection for folders)

The Selective Mirror function automatically generates copies of certain folders, which allows data recovery even after the loss of source data.

Add Selective Mirror List

¨ç Choose Selective Mirror activation.

¨è Pressing the add button will move the screen to add a new list.

¨é Under ¡°source path¡±, select the folder to be backed up and under ¡°destination path¡± select the folder that will save the back-up data.

¨ê Once the save button is pushed, a new list will have been added.

Edit Selective Mirror List

¨ç Checkbox the item to be edited and press the ¡®edit¡¯ button.

* Only one item can be edited at a time.

¨è Edit the ¡°source path¡± and the ¡°destination path¡± and press ¡°OK¡± to confirm the edited set-up.

Delete Selective Mirror List

¨ç Checkbox the item to be deleted.

* More than one item at a time can be deleted.

¨è Press the ¡°delete¡± button to confirm the deleted set-up.

Use Selective Mirror

If SMB and FTP is used to store data in the LG Network Storage and a change incurs in the source folder, the same change will apply to the destination folder and the source folder will be double protected.

* To maximize the effects of Selective Mirror, it is recommended to set up different volumes for the source folder and the destination folder. (for the single disks setting or the RAID 1+ linear volume setting)

Example) source folder: volume1/source destination folder: volume2/destination

* Conditions

¨ç The source folder and the destination folder cannot be the same folder.

¨è One source folder may have up to 4 destination folders.

¨é A folder designated as a source folder cannot be designated as a destination folder in another setting.

¨ê A subfolder of a source folder cannot be designated a destination folder.

¨ë A folder designated as a destination folder cannot be designated as a source folder in another setting.