Mail Notification

To use Mail Notification, the LG Network Storage usage amount can be periodically checked. Registration information and results will be sent to users subsequent to their new registration.

¨ç To configure the mail notification, click on the ¡®Edit¡¯ button.

¨è To use it check ¡®Disable¡¯ if ¡®Enable¡¯ is not used. If ¡®Enable¡¯ is checked, proceed with the following steps:

¨é SMTP Server Address: Input the Mail Server address. Refer to the information page in the network administrator Mail Service, and input the accurate SMTP Server Address value. (e.g. smtp.mail.yahoo.com) In the case that the port number used for the mail server is not the default value, the port number should be recorded next to the server address. This would generally be the case when the SMTP SSL has been designated. (e.g. smtp.gmail.com:446)

¨ê SMTP Authentication: When sending mail, dependant on the mail server, login may be required. In the case of own mail server, the SMTP Authentication must be activated. (e.g. Smtp.Webmail SMTP servers such as yahoo.com perform certification processes. Refer to the user webmail service help)

¨ë SMTP SSL Support: Some mail servers¡¯ login information is encrypted and sent. At this time the SMTP SSL Support must be activated. (e.g. Smtp.Webmail smtp servers such as gmail.com perform certification processes. Refer to the user webmail service help)

¨ì Subject: The information email subject can be specified or changed.

¨í Recipient Mail Address: Input the mail receipt administrator¡¯s address.

¨î Notification Trigger: Set up the information concerning the periodic use of the HDD. In the case of not wanting to receive message periodically, the option may be disabled.

¨ï HDD Status sending time: The HDD use information mail out frequency can be determined (daily/weekly/monthly).