Firmware

LG Network Storage firmware settings can be changed (Upgrade, Initialization, Configuration and Backup/Restore).

Upgrade

LG Network Storage system and Blu-ray/DVD Driver firmware can be downloaded from the product web site, and can be used for upgrading. Systems with a fire wall do not allow upgrades to be installed

[System Firmware Upgrade]

¨ç Verify connection to the Internet and download system firmware for the LG Network Storage from the product site linked below. ¢Ñ http://www.lge.com

¨è Press the ¡°find¡± button to select the system firmware downloaded from the product site.

¨é Press the ¡°upgrade¡± button to Install the selected system firmware to LG Network Storage. The

upgrade progress may be viewed on the LCD in the front.

¨ê When upgrade is finished, the system will automatically reboot. The web connection will be automatically terminated and therefore should be reconnected.

[Blu-ray/DVD Drive Firmware Upgrade]

¨ç Verify connection to the Internet and download the firmware for the Blu-ray/DVD drive attached to the LG Network Storage from the product site linked below.

¢Ñ http://www.lge.com

¨è Select the Blu-ray/DVD drive firmware downloaded from the product site.

¨é Install selected Blu-ray/DVD drive firmware.

¨ê When upgrade is finished, the version of installed Blu-ray/DVD drive firmware will be indicated

* For stability of data, a backup of the LG Network Storage is strongly recommended before upgrading. Installation takes between 1 to several minutes. Advance access of other client users to the LG Network Storage while upgrading firmware is forbidden.

Initialization

LG Network Storage initialization function. Clicking on the ¡®Initialization¡¯ will Initialize the system.

* Caution must be taken when changing the settings, for post Initialization all-user information and data will be deleted.

* Initialization will take about 10 minutes.

Configuration Back-up

This allows the back-up/recovery of settings for LG Network Storage at a certain time. Network settings (host name, IP address, workgroup), time setting (date/time, NTP), mail notification service setting, share administration (user, group, folder security), service setting values may be backed up but user data requires separate back-up.

[Backup]

Save the current user configuration.

* 5 backup files can be saved at maximum.

[Restore]

¨ç Select the backup file of the time point to restore.

¨è Click on the ¡®Restore¡¯ button and reconfigure the user configuration.

Save Settings to PC and Restore

During initialization of NAS, configuration files can be saved to PC for later restoration.

[Save Configuration Files to PC ]

Choose configuration files to be saved to PC and click on the ¡®Save¡¯ button to save them to PC.

[Restore NAS User Settings Saved on PC]

NAS settings can be restored using configuration files saved on the PC.

1. Choose the ¡®Restore LG Network Storage configuration from configuration file backed up in PC¡¯ menu and select from saved configuration files using ¡®Find¡¯.

2. Select the configuration file to use for restoration and click on ¡®Restore¡¯ to change NAS settings as selected.