Network Printer

The network printer can be used by connecting the USB printer to the LG Network Storage.

¨ç Select Service > Network Printer from the administrator¡¯s web menu.

¨è Check ¡°Enable¡±, click the ¡°Apply¡± button.

[Windows users]

¨ç In the web menu go to ¡°Enable¡± to connect the network printer, after which an LG Network Storage printer icon appears.

¨è Doubling clicking on the icon shows the progress of the printer driver installation. For installation issues refer to the printer manual.

¨é If installation is unsuccessful use the network printer service.

[Mac users]

¨ç Click on Go/ Utilities in the tool menu.

¨è Click on the Printer Setup Utility.

¨é Click on Add.

¨ê Hold the alt key down while clicking on More Printers.

¨ë In the pop up window:

i. Select Advanced.

ii. Select Windows Printer via SAMBA.

iii. Input the printer URI. The form name is smb: /LG Network Storage IP/printer. The printer name can be found in the Device Configuration(device config)/ USB Printer page.

iv. In Printer Model, select Generic.

v. Click Add.

* By pressing the alt key while clicking on More Printers, a range of printers can be seen. There are no other options.

vi. The printer appears in the printer list. Now the printer is ready for use.

* Linux users must consult the OS manual, or inquire at the printer company.